IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "u-100-f29ua3lh-real-listing.ifc"
Time stamp: "2026-05-09T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 Add2 — Real Listing AI Design"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE" version "1.0" identifier "bim.house" | change ADDED | created 1714000000 (2024-04-24T23:06:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "サウナのある家 — 100㎡ ととのい平屋" | long name "BIM.HOUSE" | phase "1-story 木造軸組 + 構造用合板耐力壁(壁倍率2.5) + 高断熱(UA推定0.4) + フィンランド式サウナ, 100sqm proposed for 200sqm lot at"
  IFCSITE | object type "Real listing site, 200sqm" | elevation above sea level 0.
    IFCBUILDING "サウナのある家 — 100㎡ ととのい平屋 (Proposed)" | object type "1F 木造軸組 + 構造用合板耐力壁(壁倍率2.5) + 高断熱(UA推定0.4) + フィンランド式サウナ 100sqm" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "GF" | elevation 0.
        contains 44 elements
          1 x IFCSLAB | FLOOR | names: "F1 床スラブ" | material: "Generic" | property sets: Pset_SlabCommon, BaseQuantities
          9 x IFCWALL | names: "北 外壁(木造 構造用合板 壁倍率2.5)", "南 外壁(木造 構造用合板 壁倍率2.5)", "東 外壁" (+6 more) | material: "Generic" | property sets: Pset_WallCommon, BaseQuantities
          1 x IFCROOF | FLAT_ROOF | names: "屋根(ガルバ片流れ・断熱200)" | material: "Generic" | property sets: Pset_RoofCommon, BaseQuantities
          13 x IFCFURNISHINGELEMENT | names: "サウナベンチ 2段(アスペン材)", "サウナストーブ(対流式)", "外気浴ウッドデッキ(屋外・開放/建築面積非算入)" (+10 more) | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities
          9 x IFCWINDOW | names: "サウナ窓(外気浴ビュー)", "南面 大開口(LDK)", "寝室 東窓" (+6 more) | material: "Generic" | property sets: Pset_WindowCommon, BaseQuantities
          6 x IFCSANITARYTERMINAL | names: "シャワー", "洗面化粧台", "水風呂(冷水プランジ)" (+3 more) | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities
          1 x IFCDOOR | names: "玄関ドア" | material: "Generic" | property sets: Pset_DoorCommon, BaseQuantities
          2 x IFCFLOWTERMINAL | names: "ロスナイ 24h 第一種熱交換換気(給排気1)", "24h換気 第一種熱交換(給排気2)" | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities
          2 x IFCSHADINGDEVICE | names: "深い軒(南・夏日射制御/冬取得)", "外気浴 目隠し木ルーバー(プライバシー)" | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "F1 床スラブ" (IFCLABEL)
  BaseQuantities | quantities | on 4 objects (2 IFCFLOWTERMINAL, 2 IFCSANITARYTERMINAL)
    NetVolume = 0.1080 [CUBIC_METRE]
  BaseQuantities | quantities | on 3 objects (3 IFCWALL)
    Height = 2.7000 [MILLI METRE]
    Length = 0.1500 [MILLI METRE]
    NetSideArea = 0.4050 [SQUARE_METRE]
    NetVolume = 3.2400 [CUBIC_METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCWALL)
    Height = 2.7000 [MILLI METRE]
    Length = 12.5000 [MILLI METRE]
    NetSideArea = 33.7500 [SQUARE_METRE]
    NetVolume = 5.0625 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    NetArea = 100.0000 [SQUARE_METRE]
    NetVolume = 15.0000 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCROOF)
    NetArea = 100.0000 [SQUARE_METRE]
    NetVolume = 22.0000 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 2.7000 [MILLI METRE]
    Length = 4.7000 [MILLI METRE]
    NetSideArea = 12.6900 [SQUARE_METRE]
    NetVolume = 1.9035 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 2.3000 [MILLI METRE]
    Length = 0.1500 [MILLI METRE]
    NetSideArea = 0.3450 [SQUARE_METRE]
    NetVolume = 0.8798 [CUBIC_METRE]
  BaseQuantities | quantities | on 1 object (1 IFCWALL)
    Height = 2.3000 [MILLI METRE]
    Length = 2.5500 [MILLI METRE]
    NetSideArea = 5.8650 [SQUARE_METRE]
    NetVolume = 0.8798 [CUBIC_METRE]
  BaseQuantities: 30 more contents on 30 objects not shown
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "北 外壁(木造 構造用合板 壁倍率2.5)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "南 外壁(木造 構造用合板 壁倍率2.5)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "東 外壁" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "西 外壁" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "間仕切り耐力壁 (LDK / プライベート)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "間仕切り (寝室 / 水まわり)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "サウナ室 西壁(断熱・気密)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "サウナ室 南壁(断熱・気密)" (IFCLABEL)
  Pset_WallCommon: 1 more content on 1 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 100.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "屋根(ガルバ片流れ・断熱200)" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "サウナベンチ 2段(アスペン材)" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "サウナストーブ(対流式)" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCSANITARYTERMINAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "シャワー" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCSANITARYTERMINAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "洗面化粧台" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "外気浴ウッドデッキ(屋外・開放/建築面積非算入)" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCSANITARYTERMINAL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "水風呂(冷水プランジ)" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ととのいチェア ×2" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "アイランドキッチン" (IFCLABEL)
  Pset_BuildingElementCommon: 15 more contents on 15 objects not shown
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "サウナ窓(外気浴ビュー)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面 大開口(LDK)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "寝室 東窓" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "寝室 南窓(掃出し)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "LDK 西窓" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "LDK 南窓 2" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "星見トップライト(天窓・ととのい上部)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "ハイサイドライト(北・安定昼光)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon: 1 more content on 1 objects not shown
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "玄関ドア" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)