IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "bim.house catalog product — reference values, verify with manufacturer"
File name: "EVOLTZ-B5-STD.ifc"
Time stamp: "2026-01-01T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 — bim.house product catalog"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE catalog export" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE catalog export" version "1.0" identifier "bim.house" | change ADDED | created 1767225600 (2026-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "evoltz B5 木造用油圧式制振装置 (evoltz)" | long name "BIM.HOUSE" | phase "Catalog product reference model"
  IFCSITE "Catalog Context" | elevation above sea level 0.
    IFCBUILDING "Catalog Building" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Level" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | names: "evoltz B5 木造用油圧式制振装置" | descriptions: "木造軸組工法・2×4工法対応の油圧式制振ダンパー。ドイツBILSTEIN社製造。世界3カ国特許のバイリニア特性により、震度1の微小振動から大規模地震まで対応。地震の揺れを最大50%軽減。100万回作動試験クリア。設計耐用年数60年のメンテナンスフリー設計。" | property sets: Pset_bimhouse_Catalog

Property sets
  Pset_bimhouse_Catalog | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "evoltz" (IFCLABEL)
    ManufacturerURL = "https://www.evoltz.com/" (IFCLABEL)
    Reference = "EVOLTZ-B5-STD" (IFCLABEL)
    WarrantyYears = 60 (IFCINTEGER)
    spec_applicable_structure = "["木造軸組工法","2×4工法"]" (IFCLABEL)
    spec_bilstein_oem = "true" (IFCLABEL)
    spec_cycles_tested = "1000000" (IFCLABEL)
    spec_damper_type = "油圧式" (IFCLABEL)
    spec_design_life_years = "60" (IFCLABEL)
    spec_maintenance = "不要（メンテナンスフリー）" (IFCLABEL)
    spec_noto_earthquake_2024 = "573棟中 倒壊・全壊・半壊ゼロ" (IFCLABEL)
    spec_operating_temp_max_c = "80" (IFCLABEL)
    spec_operating_temp_min_c = "-20" (IFCLABEL)
    spec_patent_countries = "3" (IFCLABEL)
    spec_seismic_reduction_pct = "50" (IFCLABEL)
    spec_supply_records = "33000" (IFCLABEL)