IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "bim.house catalog product — reference values, verify with manufacturer"
File name: "SCHUECO-AWS-90.ifc"
Time stamp: "2026-01-01T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 — bim.house product catalog"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE catalog export" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE catalog export" version "1.0" identifier "bim.house" | change ADDED | created 1767225600 (2026-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "AWS 90 アルミ高断熱 (Schüco)" | long name "BIM.HOUSE" | phase "Catalog product reference model"
  IFCSITE "Catalog Context" | elevation above sea level 0.
    IFCBUILDING "Catalog Building" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Level" | elevation 0.
        contains 1 element
          1 x IFCWINDOW | names: "AWS 90 アルミ高断熱" | descriptions: "Schüco AWS 90 アルミ高断熱窓。U値1.9、η値0.49の高断熱性能を誇り、JISグレードF☆☆☆☆の安全性を確保。10年保証付き。" | property sets: Pset_bimhouse_Catalog

Property sets
  Pset_bimhouse_Catalog | properties | on 1 object (1 IFCWINDOW)
    JIS_Grade = "F☆☆☆☆" (IFCLABEL)
    ListPrice_JPY_excl_tax = 478000 (IFCINTEGER)
    Manufacturer = "Schüco" (IFCLABEL)
    Reference = "SCHUECO-AWS-90" (IFCLABEL)
    SolarHeatGainCoefficient_eta = 0.49 (IFCREAL)
    ThermalTransmittance_U = 1.90 (IFCREAL)
    WarrantyYears = 10 (IFCINTEGER)